

**Ingrams Time Systems Pty Ltd**

**ABN** 50 129 539 251 **ACN** 129 539 251

12/21 Eugene Terrace Ringwood VIC 3134 Australia

**P** 03 9876 0066 **F** 03 9876 0055 **E** sales@ingrams.com.au **W** www.ingrams.com.au

# Standard Wireless Clocks Specifications

## 300mm Dial Standard Wireless Clock Specifications



* Heavy Duty Construction
* Durable ABS Casing or Aluminium Casing
* Poly carbonate Lens (shatter resistant)
* Battery (2 D-Cell) or Electric 230 Vac
* Battery Life Expectancy – 5 years

**Rear Case Diameter:** 13.2″ (33.528cm)
**Front Case Diameter:** 12.75″ (32.385cm)
**Dial Graphics Diameter:** 12″ (30.48cm)
**Edge Thickness:** 2.6″ (6.604cm)
**Center Thickness:** 3″ (7.62cm)

## 400mm Dial Standard Wireless Clock Specifications



* Heavy Duty Construction
* Durable ABS Casing or Aluminium Casing
* Poly carbonate Lens (shatter resistant)
* Battery (2 D-Cell) or Electric 230 Vac
* Battery Life Expectancy – 5 years

**Rear Case Diameter:** 16″ (40.64cm)
**Front Case Diameter:** 15.5″ (39.37cm)
**Dial Graphics Diameter:** 14.5″ (36.83cm)
**Edge Thickness:** 2.25″ (5.715cm)
**Center Thickness:** 2.75” (6.985cm)
**Ceiling and Side Mount Dimensions:** 3″ H x 4.5″ D (3.62cm H x 11.43cm D)

## 300mm (33.02cm) and 400mm (40.64cm) Rear View





Standard Wireless Clock



Aluminium Wireless Clock